Nome: Ernesto Gurgel Valente Neto, Matricula:1010157.  
  
1. Liste os diferentes protocolos que aparecem na coluna Protocol na janela de

listagem de pacotes após o passo 7;

HTTP, HTTP/XML, OCSP

2. Quanto tempo passou de quando a mensagem HTTP GET foi enviada até que a resposta OK foi recebida? (por *default*, o valor da coluna Time na janela de listagem de pacotes é a quantidade de tempo, em segundos, desde que a captura iniciou). Para exibir o campo Time no formato hora do dia, selecione o menu View, depois Time Display Format, então selecione Time of day.

PEDIDO: 20:58:04,19

RESPOSTA: 20:58:04,70

3. Qual é o endereço IP do site www.aw.com? Qual é o endereço IP da interface de rede do seu computador?

REDE IP: 172.17.28.16

SITE IP: 62.109.43.157

4. imprima as mensagens HTTP GET e a resposta a ela (HTTP/1.1 200 OK). Para fazer isso, selecione Print no menu File, e depois “Selected Packet Only” e “Print as Displayed”. Ok (ou Imprimir) para confirmar.

1866 2019-09-04 20:58:04,199363 172.17.28.16 62.109.43.157 HTTP 496 GET /kurose\_br HTTP/1.1 Frame 1866: 496 bytes on wire (3968 bits), 496 bytes captured (3968 bits) on interface 0 Ethernet II, Src: Dell\_a5:28:f1 (d0:94:66:a5:28:f1), Dst: Fortinet\_09:01:02 (00:09:0f:09:01:02) Internet Protocol Version 4, Src: 172.17.28.16, Dst: 62.109.43.157 Transmission Control Protocol, Src Port: 56158, Dst Port: 80, Seq: 1, Ack: 1, Len: 442 Hypertext Transfer Protocol

1946 2019-09-04 20:58:04,705481 62.109.43.157 172.17.28.16 HTTP 429 HTTP/1.1 301 Moved Permanently (text/html) Frame 1946: 429 bytes on wire (3432 bits), 429 bytes captured (3432 bits) on interface 0 Ethernet II, Src: Fortinet\_09:01:02 (00:09:0f:09:01:02), Dst: Dell\_a5:28:f1 (d0:94:66:a5:28:f1) Internet Protocol Version 4, Src: 62.109.43.157, Dst: 172.17.28.16 Transmission Control Protocol, Src Port: 80, Dst Port: 56158, Seq: 1, Ack: 443, Len: 375 Hypertext Transfer Protocol Line-based text data: text/html